//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//

Command ID:	VOCODER_SEL
Send	Command: 84 A9 61 00 02 00 10 01
Receive	Command:84 A9 61 00 02 00 10 00
Pause 3000
Command ID:	CODEC_SELECT
//Send	Command: 84 A9 61 00 02 03 2D 02
Send	Command: 84 A9 61 00 02 03 2D {CODEC_VAR}
Receive	Command:84 A9 61 00 02 03 2D 00
Pause 200
Command ID:	CALL_OPTION
//Send	Command: 84 A9 61 00 06 05 47 f1 00 00 00 00
Send	Command: 84 A9 61 00 06 05 47 {OPTION_VAR1} {OPTION_VAR2} 00 00 00
Receive	Command:84 A9 61 00 02 05 47 00
Pause 2000
Command ID:	 Select RF frequency, 409.750 Hz
Send	Command: 84 A9 61 00 06 00 6A E2 29 02 00 68
Receive	Command:84 A9 61 00 02 00 6A 00
Command ID:	 Select RF frequency1 2R 15C6
Send	Command: 84 A9 61 00 06 00 6A E2 2a 02 7F 90
Receive	Command:84 A9 61 00 02 00 6A 00
Command ID:Set DC OFFSET!
Send	Command: 84 A9 61 00 0D 00 39 00 00 00 00 00 00 {OFFSET_VAR1} 00 08 00 {OFFSET_VAR2} 00 00
 Receive	Data:84 A9 61 00 02 00 39 00

Command ID:	MODEL_SEL    CONNECT 3700 SET 50 CONNECT 3920 SET 10 at DPMR 1847 
Send	Command: 84 A9 61 00 02 00 2B {MODEL_VAR}
Receive	Data:84 A9 61 00 02 00 2B 00
Pause 1000