//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//

//Command ID:	PROCESS_MODE
//Send	Command: 84 A9 61 00 02 00 1A 80
//Receive	Data:84 A9 61 00 02 00 1A 00
//pause 200
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100

Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100

Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100

Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100

Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100

Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100

Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100

Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100

Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100

Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100

Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100

Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100


Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 15
PAUSE 980
Button INT0
PAUSE 20
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Pause 100





Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100

Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100

Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100

Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100

Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 16
Button NIMI
Receive	Command:84 A9 61 00 02 20 17 01
PAUSE 100











